
         ________________________________________________________
        |                                                        |
        |  =====           PHILIPS SEMICONDUCTEURS               |
        | | P   |                                                |
        | |  S  |             2 Rue de la Girafe                 |
        | |   C |                  BP 5120                       |
        |  =====             14079 CAEN CEDEX 5                  |
        |                                                        |
        |________________________________________________________|


        BOARD       : PCB1643   IND : 1.0     STUDY : PN531_HSU

        PROJECT     : TAMA           DATE  : 21 Octobre 2005

        DESIGNED BY : ducastel

                                                                          
                       ***  COMPONENTS LISTE  ***                         


REFERENCE    GEOMETRY          VALUE                       SPECIFICATION         
---------    --------          -----                       -------------   


  C1         taj_r           10uF_6.3V            AVX:TAJR106K006,Tantal,Capacitor,Package:R,10%
  C2         taj_r           1.5uF_10V            AVX:TAJR155K010,Tantal,Capacitor,Package:R,10%
  C3         c0402           N.C.                 Capacitor,CER2,0402,***NOT,CONNECTED***
  C4         c0402           N.C.                 Capacitor,CER2,0402,***NOT,CONNECTED***
  C5         c0402           18pF                 Capacitor,CER2,0402,C0G,50V,5%
  C6         c0402           18pF                 Capacitor,CER2,0402,C0G,50V,5%
  C7         c0402           22pF                 Capacitor,CER2,0402,C0G,50V,5%
  C8         c0402           22pF                 Capacitor,CER2,0402,C0G,50V,5%
  C9         c0402           N.C.                 Capacitor,CER2,0402,***NOT,CONNECTED***
  C10        c0402           N.C.                 Capacitor,CER2,0402,***NOT,CONNECTED***
  C11        c0402           56pF                 Capacitor,CER2,0402,C0G,50V,5%
  C12        c0402           56pF                 Capacitor,CER2,0402,C0G,50V,5%
  C13        c0402           1nF                  Capacitor,CER2,0402,X7R,50V,10%
  C14        c0402           0.1uF                Capacitor,CER2,0402,X7R,16V,-10+10%,PDC
  C15        c0402           0.1uF                Capacitor,CER2,0402,X7R,16V,-10+10%,PDC
  C16        c0603           4.7uF                Capacitor,CER2,0603,X5R,6.3V,10%
  C17        c0603           10uF                 Capacitor,CER2,0603,X5R,4V,10%
  C18        c0603           10uF                 Capacitor,CER2,0603,X5R,4V,10%
  C19        c0402           0.1uF                Capacitor,CER2,0402,X7R,16V,-10+10%,PDC
  C20        c0402           0.1uF                Capacitor,CER2,0402,X7R,16V,-10+10%,PDC
  C21        c0402           0.1uF                Capacitor,CER2,0402,X7R,16V,-10+10%,PDC
  C22        c0402           0.1uF                Capacitor,CER2,0402,X7R,16V,-10+10%,PDC
  C23        c0402           0.1uF                Capacitor,CER2,0402,X7R,16V,-10+10%,PDC
  C24        c0402           0.1uF                Capacitor,CER2,0402,X7R,16V,-10+10%,PDC
  C25        c0402           0.1uF                Capacitor,CER2,0402,X7R,16V,-10+10%,PDC
  C26        c0402           0.1uF                Capacitor,CER2,0402,X7R,16V,-10+10%,PDC
  C27        c0402           0.1uF                Capacitor,CER2,0402,X7R,16V,-10+10%,PDC
  C28        c0402           0.1uF                Capacitor,CER2,0402,X7R,16V,-10+10%,PDC
  C29        c0402           220pF_C0G            Capacitor,CER2,0402,C0G,50V,GPR15_5C_1H_221
  C30        c0402           220pF_C0G            Capacitor,CER2,0402,C0G,50V,GPR15_5C_1H_221
  D1         topled          HSMS_A100_L100J1     AGILENT:Red,LED,Topled,30mA
  D2         to269aa         MB2S                 GENERAL_SEMICONDUTOR:SMD,Bridge,Rectifier,200V,0.5A
  D3         sod80           BAS85                PHILIPS:Schottky,Barrier,Diode,30V,0.2A
  IC1        mlf6x40_0.5     TAMA                 tama
  IC2        sot223          TS2940CW_3.3         TSC:Ultra-Low,Dropout,Fixed,Positive,voltage,Regulator,3.3V,1A,SOT223
  IC3        sot403_1        ADM3202ARU           ANALOG-DEVICES:Low,Power,3.3V,RS232,Line-Driver,Receiver,Package:TSSOP16
  J1         subd_09fc       D09S13A4GL00         FCI:Delta-D,Connector,Right-Angle,Female,Norm,HE5
  J2         jack2.5_h       JACK2.5_H            CLIFF:DC10B,Power,Connector,Horizontal,2.5mm
  J3         5108_2x14s_0.8md 5108_1_02810_00      WP-PRODUCTS:5108,Serie,SMT,Connector,Straight,Male,2x14pins,0.8mm
  L1         self_mlf2012    0.56uH               TDK:MLF2012DR56K,Chip,Inductor,SMD,0.15A,10%
  L2         self_mlf2012    0.56uH               TDK:MLF2012DR56K,Chip,Inductor,SMD,0.15A,10%
  R1         r0402           A DEFINIR            Resistor,Package:0402,***TO,BE,DEFINE***
  R2         r0402           A DEFINIR            Resistor,Package:0402,***TO,BE,DEFINE***
  R3         r0402           A DEFINIR            Resistor,Package:0402,***TO,BE,DEFINE***
  R4         r0402           A DEFINIR            Resistor,Package:0402,***TO,BE,DEFINE***
  R5         r0402           0                    Resistor,Package:0402,5%,1/16W
  R6         r0402           0                    Resistor,Package:0402,5%,1/16W
  R7         r0402           0                    Resistor,Package:0402,5%,1/16W
  R8         r0402           0                    Resistor,Package:0402,5%,1/16W
  R9         r0402           820                  Resistor,Package:0402,5%,1/16W
  R10        r0402           1K                   Resistor,Package:0402,5%,1/16W
  R11        r0402           2.7K                 Resistor,Package:0402,5%,1/16W
  R12        r0402           47K                  Resistor,Package:0402,5%,1/16W
  R13        r0402           47K                  Resistor,Package:0402,5%,1/16W
  R14        r0402           47K                  Resistor,Package:0402,5%,1/16W
  R15        r0402           47K                  Resistor,Package:0402,5%,1/16W
  R16        r0402           47K                  Resistor,Package:0402,5%,1/16W
  R18        r0402           100K                 Resistor,Package:0402,5%,1/16W
  R19        r0402           3.3_1%               Resistor,Package:0402,1%,1/16W
  R20        r0402           3.3_1%               Resistor,Package:0402,1%,1/16W
  ST1        chevron_a       CHEVRON              ***NOT,CONNECTED***
  ST2        chevron_a       CHEVRON              ***NOT,CONNECTED***
  ST3        chevron_a       CHEVRON              ***NOT,CONNECTED***
  ST4        chevron_a       CHEVRON              ***NOT,CONNECTED***
  ST5        chevron_a       CHEVRON              ***NOT,CONNECTED***
  ST6        chevron_a       CHEVRON              ***NOT,CONNECTED***
  ST7        chevron_a       CHEVRON              ***NOT,CONNECTED***
  ST8        chevron_a       CHEVRON              ***NOT,CONNECTED***
  ST9        chevron_a       CHEVRON              ***NOT,CONNECTED***
  ST10       chevron_a       CHEVRON              ***NOT,CONNECTED***
  TB1        bar2sp          CAVAL_2.54           Pattern,Single,Row,2,pin,+,ANTELEC,CCM1D
  TB2        bar2sp          Empr_CAVAL_2.54      Pattern,Single,Row,2,pin
  TB3        bar2sp          CAVAL_2.54           Pattern,Single,Row,2,pin,+,ANTELEC,CCM1D
  TB4        bar2sp          CAVAL_2.54           Pattern,Single,Row,2,pin,+,ANTELEC,CCM1D
  TB5        bar2sp          CAVAL_2.54           Pattern,Single,Row,2,pin,+,ANTELEC,CCM1D
  TB6        bar2sp          CAVAL_2.54           Pattern,Single,Row,2,pin,+,ANTELEC,CCM1D
  TB7        bar2sp          CAVAL_2.54           Pattern,Single,Row,2,pin,+,ANTELEC,CCM1D
  TB8        tp0.9           CAVAL_2.54           Pattern,Single,Row,1,pin,+,ANTELEC,CCM1D
  TB9        tp0.9           CAVAL_2.54           Pattern,Single,Row,1,pin,+,ANTELEC,CCM1D
  TB10       tp0.9           CAVAL_2.54           Pattern,Single,Row,1,pin,+,ANTELEC,CCM1D
  TB12       tp0.9           CAVAL_2.54           Pattern,Single,Row,1,pin,+,ANTELEC,CCM1D
  TB13       tp0.9           CAVAL_2.54           Pattern,Single,Row,1,pin,+,ANTELEC,CCM1D
  TB14       tp0.9           CAVAL_2.54           Pattern,Single,Row,1,pin,+,ANTELEC,CCM1D
  TB15       tp0.9           CAVAL_2.54           Pattern,Single,Row,1,pin,+,ANTELEC,CCM1D
  TB16       tp0.9           CAVAL_2.54           Pattern,Single,Row,1,pin,+,ANTELEC,CCM1D
  TB17       tp0.9           Empr_CAVAL_2.54      Pattern,Single,Row,1,pin
  TB18       tp0.9           Empr_CAVAL_2.54      Pattern,Single,Row,1,pin
  TB19       tp0.9           Empr_CAVAL_2.54      Pattern,Single,Row,1,pin
  TB21       tp0.9           Empr_CAVAL_2.54      Pattern,Single,Row,1,pin
  TB22       tp0.9           Empr_CAVAL_2.54      Pattern,Single,Row,1,pin
  TB23       tp0.9           Empr_CAVAL_2.54      Pattern,Single,Row,1,pin
  TB24       tp0.9           Empr_CAVAL_2.54      Pattern,Single,Row,1,pin
  TB25       tp0.9           Empr_CAVAL_2.54      Pattern,Single,Row,1,pin
  TP1        plage.75        PLAGE.75             ***NOT,CONNECTED***
  TP2        plage.75        PLAGE.75             ***NOT,CONNECTED***
  TP3        plage.75        PLAGE.75             ***NOT,CONNECTED***
  TP4        plage.75        PLAGE.75             ***NOT,CONNECTED***
  TP5        tpboucle1.0     5001                 KEYSTONE:Black,Testpoint,Type1
  Y1         tas3225         27.12MHZ             TOKYO-DENPA:TAS-3225A,Type,Quartz,Crystal,SMD


















